FLOW CHART FOR HEAT CONTROLLER

START

BUTTON ON

Presence of Passenger

no

Heat off

Heat on

If temprature is more than the required

Provide the required amount of heat/temperature

jjGet/sense the temperature

NO YES